|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Label | Origin (A) | Destination (B) | Length | Cable Type | TermA | TermB |
| DC Supply | K5 (Internal 12vDC PCB) | DCIN S1 Board | 1m | DC Cable 12VDC5A Rating | J Type ? | DC Barrel Jack |
| Display Loom | S1 | Touch Display | 2m | Multiply types. HDMI and USB must be shielded and possible ferrite choke on USB run. DC Cable must be 12VDC2A rated | 1 x HDMI  1 x USB A  1 x DC Barrell Jack | 1 x HDMI  1 x USB A  1 x DC Barrell Jack |
| RGB 1 | S1 | RGB Halo | 2m | 4 core ribbon or round type cable | 4 Pin Molex | Bare ends (Will terminate with crimp, or screw terminal) |
| RGB 2 | S1 | RGB Strip | 2m | 4 core ribbon or round type cable | 4 Pin Molex | Bare ends (Will terminate with crimp, or screw terminal) |
| Speaker | S1 | L & R speeakers | 2m | 2 x figure 8 speaker cable | 4 Pin Molex | Bare ends |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |